[image: image4.png]penMV

7.






https://openmv.io                                                                                                                                    AUGUST 2018

[image: image4.png]

OpenMV LCD Shield.

1 Features

· ST7735R LCD controller.

· 1.8", 128x160 pixels, 16-bit color.

· Backlight control pin.
2 Description

The LCD Shield enables OpenMV cameras to display images captured from the image sensor. It features a 1.8" 128x160 16-bpp (RGB565) TFT LCD display with a controllable backlight.
Device Information
	PART NUMBER
	BODY SIZE (NOM)

	OPENMV-LCD-SHIELD
	1.49 in × 1.87 in




3 Applications
· Video display.

.
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4 Pin Configurations and Functions
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Pin Functions
	Pin
	Description

	Header
	No
	Name
	

	J1 Pin Configuration

	J1
	1
	P0
	SPI data in.

	
	2
	P1
	NC

	
	3
	P2
	SPI clock.

	
	4
	P3
	SPI chip select (10K pull-up)

	
	5
	P4
	NC

	
	6
	P5
	NC

	
	7
	P6
	LED control.

	
	8
	3.3
	3.3v input

	J2 Pin Configuration

	J2
	1
	RST
	NC

	
	2
	BOOT
	NC

	
	3
	SYN
	NC

	
	4
	P9
	NC

	
	5
	P8
	RS

	
	6
	P7
	RESET

	
	7
	VIN
	NC

	
	8
	GND
	GND


	5 Electrical Characteristics
	
	
	
	


5.1 
Recommended Operating Conditions
	SYMBOL
	RATINGS
	MIN
	MAX
	UNIT

	VIN
	External input supply voltage range.
	2.8
	3.3
	V

	T
	Operating Temperature
	-30
	80
	°C


6 Mechanical Information
The following information is the most current data available for the designated device. This data is subject to change without notice and without revision of this document.
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