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OpenMV WiFi Shield.

1 Features

· Certified WiFi module.

· IEEE 802.11 b/g/n up to 72Mbps
· Station mode and Soft-AP support.

· Supports IEEE 802.11 WEP/WPA2 security.
· Network protocols (DHCP/DNS)
· Secure TLS stack.

· Integrated PCB antenna.
2 Description

The WiFi Shield enables OpenMV cameras to connect to the Internet. It features an ATWINC1500 FCC Certified WiFi module which can transmit data at up to 72Mbps making it perfect for streaming video. OpenMV firmware has built-in support for controlling the WiFi Shield using the network module.
Device Information
	PART NUMBER
	BODY SIZE (NOM)

	OPENMV-WIFI-SHIELD
	1.40 in × 1.05 in




3 Applications
· MJPEG Streaming.

· Wireless programming.

.
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4 Pin Configurations and Functions
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Pin Functions
	Pin
	Description

	Header
	No
	Name
	

	J1 Pin Configuration

	J1
	1
	P0
	SPI MOSI

	
	2
	P1
	SPI MISO

	
	3
	P2
	SPI SCLK

	
	4
	P3
	SPI SS

	
	5
	P4
	NC

	
	6
	P5
	NC

	
	7
	P6
	Chip Enable

	
	8
	3.3
	3.3v input

	J2 Pin Configuration

	J2
	1
	RST
	NC

	
	2
	BOOT
	NC

	
	3
	SYN
	NC

	
	4
	P9
	NC

	
	5
	P8
	IRQ

	
	6
	P7
	RESET

	
	7
	VIN
	NC

	
	8
	GND
	GND

	J3 Pin Configuration

	J3
	1
	GND
	GND

	
	2
	RXD
	Debug UART RX

	
	3
	TXD
	Debug UART TX


	5 Electrical Characteristics
	
	
	
	


5.1 
Recommended Operating Conditions
	SYMBOL
	RATINGS
	MIN
	MAX
	UNIT

	VIN
	External input supply voltage range.
	3.0
	3.6
	V

	IOUT
	External output supply current range.
	
	500
	mA

	T
	Operating Temperature
	-40
	85
	°C


6 Mechanical Information
The following information is the most current data available for the designated device. This data is subject to change without notice and without revision of this document.
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