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OpenMV-F7 A Python programmable machine vision camera.

1 Features

· 32-Bit Arm Cortex-M7 operating at 216MHz.
· High bandwidth 512KB SRAM / 2MB FLASH. 

· Double-precision Floating Point Unit (FPU),

     Full DSP instructions.

· 2 UARTs, 2 I2C, 1 SPI, 1 CAN, 3 TIM/PWM.
· 1 USB full speed (FS) for programming.
· 1 RGB LED and 2 IR LEDS on board.

· 1 uSD Card socket (supports up to 32GBs).
· Less than 150-mA power consumption.
· OV7725 image sensor (640x480, 120FPS).



2 Description

The OpenMV cameras are low-power, Python3 programmable machine vision cameras that support an extensive set of image processing functions and neural networks.

OpenMV cameras are programmed using a cross-platform IDE which allows viewing the camera's frame buffer, accessing sensor controls, uploading scripts to the camera via serial over USB (or WiFi/BLE if available).
The OpenMV-F7 camera is based on the STM32F7 Arm Cortex-M7 MCU operating at 216MHz and featuring 512KB SRAM, 2MB FLASH, FPU, DSP. Additionally, the OpenMV-F7 camera features a high sensitivity OmniVision image sensor for low-light operations.

Device Information

	PART NUMBER
	BODY SIZE (NOM)

	OPENMV-F7
	1.4 in × 1.75 in




3 Applications
· Home automation.

· Robot guidance.
· Industrial Applications.
· Surveillance Applications.

· Object detection and tracking.
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4 Pin Configurations and Functions
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Pin Functions
	Pin
	Description

	Header
	No
	Name
	

	J1 Pin Configuration

	J1
	1
	P0
	UART1 RX – TM1 CH3N – SPI 2 MOSI

	
	2
	P1
	UART1 TX – TM1 CH2N – SPI 2 MISO

	
	3
	P2
	CAN2 TX – TM1 CH1N – SPI 2 SCLK

	
	4
	P3
	CAN2 RX – SPI 2 SS

	
	5
	P4
	TIM2 CH3 – I2C 2 SCL – UART 3 TX

	
	6
	P5
	TIM2 CH4 – I2C 2 SDA – UART3 RX

	
	7
	P6
	TIM2 CH1 – DAC – ADC

	
	8
	3.3
	3.3V Rail (250 mA Supply MAX).

	J2 Pin Configuration

	J2
	1
	RST
	Reset (Connect to GND to reset).

	
	2
	BOOT
	Boot 0 (Connect to 3.3V for DFU mode).

	
	3
	SYN
	Frame synchronization pin (Use to frame sync cams).

	
	4
	P9
	Servo3 – TIM4 CH3

	
	5
	P8
	Servo2 – TIM4 CH2 – I2C4 SDA

	
	6
	P7
	Servo1 – TIM4 CH1 – I2C4 SCL

	
	7
	VIN
	VIN (3.6V – 5V).

	
	8
	GND
	GND Rail

	J3 Pin Configuration

	J3
	1
	SWC
	Serial wire debug clock.

	
	2
	SWD
	Serial wire debug data.

	
	3
	RST
	Reset (active low).

	
	4
	3.3V
	3.3V rail (250 mA Supply MAX)

	
	5
	GND
	GND rail


	5 Electrical Characteristics
	
	
	
	

	5.1 
Absolute Maximum Ratings1
	
	
	

	
	
	
	

	SYMBOL
	RATINGS
	MIN
	MAX
	UNIT

	VIN
	External input supply voltage range.
	3.6
	5.5
	V

	VOUT
	External output supply voltage range.
	
	3.3
	

	VI/O
	Input voltage range on ADC/DAC pins.
	-0.3
	4.0
	

	
	Input voltage range on any other pins.
	-0.3
	7.3
	

	IOUT
	External output supply current range.
	
	300
	mA

	II/O
	Output current sunk by any I/O and control pin
	
	25
	

	
	Output current sourced by any I/O and control pin
	
	-25
	

	ΣII/O
	Total output current sunk by all I/Os and control pins
	
	120
	mA


	
	Total output current sourced by all I/Os and control pins
	
	120
	

	TJ
	Junction temperature.
	
	125
	°C

	Tstq
	Storage temperature.
	-65
	150
	

	
	
	
	
	


5.2 
Recommended Operating Conditions
	SYMBOL
	RATINGS
	MIN
	MAX
	UNIT

	VIN
	External input supply voltage range.
	3.6
	5.0
	V

	VOUT
	External output supply voltage range.
	
	3.3
	

	VI/O
	Input voltage range on ADC/DAC pins.
	-0.3
	3.6
	

	
	Input voltage range on any other pins.
	-0.3
	5.0
	

	IOUT
	External output supply current range.
	
	500
	mA

	TJ
	Junction temperature.
	-40
	125
	°C


(1) Stresses beyond those listed under Absolute Maximum Ratings may cause permanent damage to the device. These are stress ratings only, which do not imply functional operation of the device at these or any other conditions beyond those indicated under Recommended Operating Conditions. Exposure to absolute-maximum-rated conditions for extended periods may affect device reliability.
6 Mechanical Information
The following information is the most current data available for the designated device. This data is subject to change without notice and without revision of this document.
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