<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="35.6" y2="0" width="0" layer="20"/>
<wire x1="35.6" y1="0" x2="35.6" y2="26.67" width="0" layer="20"/>
<wire x1="35.6" y1="26.67" x2="0" y2="26.67" width="0" layer="20"/>
<wire x1="0" y1="26.67" x2="0" y2="0" width="0" layer="20"/>
<text>https://openmv.io</text>
<text>OpenMV</text>
<text>CAN/RS232 Shield R1</text>
<text>4.7.23</text>
<text>GND</text>
<text>CAN
RS232
Shield
R1</text>
<text>RAW</text>
<text>GND</text>
<text>FSYNC
P10</text>
<text>GND</text>
<text>PWR</text>
<text>AIN</text>
<text>SYN</text>
<text>CH</text>
<text>CL</text>
<text>TRM</text>
<text>TRM</text>
<text>CTX
P1</text>
<text>CTX
P2</text>
<text>CRX
P3</text>
<text>TX</text>
<text>RX</text>
<text>VIN</text>
<text>TXO
P4</text>
<text>RXI
P5</text>
<text>ADC
P6</text>
<text>O</text>
<text>I</text>
<text>mA</text>
<text>PWR - 6V to 36V </text>
<text>AIN - 0 to 5V or 4-20mA</text>
<text>SYN - 0 to 5V I/O</text>
</plain>
<libraries>
<library name="openmv">
<packages>
<package name="ROHS">
</package>
<package name="OPENMV-LOGO">
</package>
<package name="WEEE">
</package>
<package name="OMV-LOGO">
</package>
</packages>
</library>
<library name="openmv5">
<description>Generated from &lt;b&gt;poe.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="OPENMV5-TOP">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Aesthetics&lt;/h3&gt;
This library contiains non-functional items such as logos, build/ordering notes, frame blocks, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="FIDUCIAL-1X2">
<description>&lt;h3&gt;Fiducial - Circle, 1mm&lt;/h3&gt;
&lt;p&gt;Point-of-reference for pick-and-place machines and other optical instruments.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;FIDUCIAL&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="sfe">
<packages>
<package name="0402-RES">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="0402-CAP">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C0402">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="CPDQT5V0HE-HF">
<description>&lt;ESD Suppressors / TVS Diodes DIODE ESD 5VWM 65W 0402/SOD-923F&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="CPDQT5V0HEHF">
<description>&lt;b&gt;CPDQT5V0HE-HF-2&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
<description>&lt;p&gt;&lt;b&gt;Generic 2012 (0805) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="rcl">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
http://www.secc.co.jp/pdf/os_e/2004/e_os_all.pdf &lt;b&gt;(SANYO)&lt;/b&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;

&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="TPS613222ADBVR">
<description>&lt;6-uA Quiescent Current, 1.8-A Switch Current Boost Converter&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="SOT95P280X145-5N">
<description>&lt;b&gt;DBV (R-PDSO-G5)&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="MAKK2016T2R2M">
<packages>
<package name="INDC2016X100N">
</package>
</packages>
</library>
<library name="1771088">
<description>&lt;PCB terminal block, nominal current: 6 A, rated voltage (III/2): 160 V, nominal cross section: 0.5 mm?, Number of potentials: 8, Number of rows: 1, Number of positions per row: 8, product range: PTSM 0,5/..-H-SMD, pitch: 2.5 mm, connection method: Push-in spring connection, mounting: SMD soldering, conductor/PCB connection direction: 0 ?, color: black, Pin layout: Linear pad geometry, type of packaging: packed in cardboard&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="1771088">
<description>&lt;b&gt;1771088&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="FM240A">
<description>&lt;Diodes - General Purpose, Power, Switching GP Si Rectifier SMB,2A,40V&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="DIOM5025X231N">
<description>&lt;b&gt;DO-214AC&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="74LVC1G17SE-7">
<description>&lt;DiodesZetex 74LVC1G17SE-7, Buffer, Push-Pull, Non-Inverting, 1.65  5.5 V, 5-Pin SOT-353&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="SOT65P210X110-5N">
<description>&lt;b&gt;SOT353-&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="AP64060WU-7">
<description>&lt;Switching Voltage Regulators DCDC Conv HV Buck TSOT26(STD) T&amp;R 3K&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="SOT95P280X100-6N">
<description>&lt;b&gt;TSOT26 AP62300&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="NRS4018T100MDGJ">
<description>&lt;Fixed Inductors 4018 10uH 180mOhms +/-20%Tol 1200mA&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="NRS4018T100MDGJ">
<description>&lt;b&gt;(NR series S type)&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="SMAJ40CAe3_TR13">
<description>&lt;ESD Suppressors / TVS Diodes TVS&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="SMAJ40CAE3TR13">
<description>&lt;b&gt;SMAJ40CAe3/TR13-2&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="SSM3J356R_LF">
<description>&lt;MOSFET Small-signal MOSFET ID: -2A, VDSS: -60V&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="SOTFL95P240X88-3N">
<description>&lt;b&gt;SOT-23F&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="MMSZ5231B-7-F">
<description>&lt;Zener Diode 5.1V 5% 500mW SOD123 Diodes Inc MMSZ5231B-7-F Zener Diode, 5.1V 5% 0.5 W SMT 2-Pin SOD-123&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="SOD3716X145N">
<description>&lt;b&gt;SOD123-ren1&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="SparkFun-Jumpers">
<description>&lt;h3&gt;SparkFun Jumpers&lt;/h3&gt;
In this library you'll find jumpers, or other semipermanent means of changing current paths. The least permanent form is the solder jumper. These can be changed by adding, removing, or moving solder. In cases that are less likely to be changed we have jumpers that are connected with traces. These can be cut with a razor, or reconnected with solder. Reference designator JP.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMT-JUMPER_2_NC_PASTE_SILK">
</package>
<package name="SMT-JUMPER_3_1-NC_PASTE_SILK">
</package>
<package name="SMT-JUMPER_2_NO_SILK">
</package>
</packages>
</library>
<library name="74LVC1G07GW_125">
<description>&lt;74LVC1G07 - Buffer with open-drain output@en-us&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="SOT65P212X110-5N">
<description>&lt;b&gt;TSSOP5&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="MCP2542FD-E_SN">
<description>&lt;Microchip MCP2542FD-E/SN, CAN Transceiver 8Mbit/s 1-Channel CAN, ISO 11898-2, ISO 11898-5, ISO/DIS11898-2, 8-Pin SOIC&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="SOIC127P600X175-8N">
<description>&lt;b&gt;MCP2542WFDT-E/SN&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Discrete Semiconductors&lt;/h3&gt;
This library contains diodes, optoisolators, TRIACs, MOSFETs, transistors, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-3">
<description>SOT23-3</description>
</package>
</packages>
</library>
<library name="SRF4532-110Y">
<description>&lt;Bourns Type 4532 Wire-wound SMD Inductor with a Ferrite Core, 11 uH -30  +50% Wire-Wound 300mA Idc&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="SRF4532101Y">
<description>&lt;b&gt;SRF4532&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="SN65C3221EPWR">
<description>&lt;3-V To 5.5-V Single Channel RS-232 1 Mbit/s Line Driver/Receiver&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="SOP65P640X120-16N">
<description>&lt;b&gt;PW0016A&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="LM321LVIDCKR">
<description>&lt;1-Channel industry standard low voltage operational amplifier&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="SOT65P210X110-5N">
<description>&lt;b&gt;DCK (R-PDSO-G5)&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="MM3Z3V6T1G">
<description>&lt;ON Semiconductor MM3Z3V6T1G Zener Diode, 3.6V 5% 200 mW SMT 2-Pin SOD-323&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="SOD2512X110N">
<description>&lt;b&gt;SOD-323 - case 477-02 - issue H&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="openmv5" package="OPENMV5-TOP" value="OPENMV5-TOP"/>
<element name="U$9" library="openmv" package="OPENMV-LOGO" value="OPENMV-LOGO"/>
<element name="U$1" library="openmv" package="WEEE" value=""/>
<element name="U$2" library="openmv" package="ROHS" value=""/>
<element name="U$3" library="openmv" package="OMV-LOGO" value=""/>
<element name="FD1" library="SparkFun-Aesthetics" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="FD2" library="SparkFun-Aesthetics" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="FD4" library="SparkFun-Aesthetics" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="FD3" library="SparkFun-Aesthetics" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="FD5" library="SparkFun-Aesthetics" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="FD6" library="SparkFun-Aesthetics" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="FD7" library="SparkFun-Aesthetics" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="FD8" library="SparkFun-Aesthetics" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="D2" library="CPDQT5V0HE-HF" package="CPDQT5V0HEHF" value="CPDQT5V0HE-HF">
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes DIODE ESD 5VWM 65W 0402/SOD-923F"/>
<attribute name="HEIGHT" value="0.42mm"/>
<attribute name="MANUFACTURER_NAME" value="Comchip Technology"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="CPDQT5V0HE-HF"/>
<attribute name="MOUSER_PART_NUMBER" value=""/>
<attribute name="MOUSER_PRICE-STOCK" value=""/>
<attribute name="MPN" value="CPDQT5V0HE-HF"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="TPS613222ADBVR" package="SOT95P280X145-5N" value="TPS613222ADBVR">
<attribute name="DESCRIPTION" value="6-uA Quiescent Current, 1.8-A Switch Current Boost Converter"/>
<attribute name="HEIGHT" value="1.45mm"/>
<attribute name="MANUFACTURER_NAME" value="Texas Instruments"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="TPS613222ADBVR"/>
<attribute name="MOUSER_PART_NUMBER" value="595-TPS613222ADBVR"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Texas-Instruments/TPS613222ADBVR?qs=W0yvOO0ixfE4d69WXsn8NQ%3D%3D"/>
<attribute name="MPN" value="TPS613222ADBVR"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0805" value="22uF">
<attribute name="MPN" value="CL21A226MQQNNNE"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08402"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0805" value="22uF">
<attribute name="MPN" value="CL21A226MQQNNNE"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08402"/>
<attribute name="VALUE"/>
</element>
<element name="L2" library="MAKK2016T2R2M" package="INDC2016X100N" value="MAKK2016T2R2M">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" 2.2 µH Shielded Drum Core, Wirewound Inductor 1.5 A 160mOhm Max 0806 (2016 Metric) "/>
<attribute name="MF" value="Taiyo Yuden"/>
<attribute name="MP" value="MAKK2016T2R2M"/>
<attribute name="MPN" value="MAKK2016T2R2M"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="2016 Taiyo Yuden"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/MAKK2016T2R2M/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="1771088" package="1771088" value="1771088">
<attribute name="DESCRIPTION" value="PCB terminal block, nominal current: 6 A, rated voltage (III/2): 160 V, nominal cross section: 0.5 mm?, Number of potentials: 8, Number of rows: 1, Number of positions per row: 8, product range: PTSM 0,5/..-H-SMD, pitch: 2.5 mm, connection method: Push-in spring connection, mounting: SMD soldering, conductor/PCB connection direction: 0 ?, color: black, Pin layout: Linear pad geometry, type of packaging: packed in cardboard"/>
<attribute name="HEIGHT" value="5.22mm"/>
<attribute name="MANUFACTURER_NAME" value="Phoenix Contact"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="1771088"/>
<attribute name="MOUSER_PART_NUMBER" value="651-1771088"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Phoenix-Contact/1771088?qs=Q77YN%2FRrsKIDMojcNKtpFQ%3D%3D"/>
<attribute name="MPN" value="1771088"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="sfe" package="0402-RES" value="100K">
<attribute name="MPN" value="AC0402FR-07100KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="sfe" package="0402-RES" value="10K">
<attribute name="MPN" value="AC0402FR-1310KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="74LVC1G17SE-7" package="SOT65P210X110-5N" value="74LVC1G17SE-7">
<attribute name="DESCRIPTION" value="DiodesZetex 74LVC1G17SE-7, Buffer, Push-Pull, Non-Inverting, 1.65  5.5 V, 5-Pin SOT-353"/>
<attribute name="HEIGHT" value="1.1mm"/>
<attribute name="MANUFACTURER_NAME" value="Diodes Inc."/>
<attribute name="MANUFACTURER_PART_NUMBER" value="74LVC1G17SE-7"/>
<attribute name="MOUSER_PART_NUMBER" value="621-74LVC1G17SE-7"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Diodes-Incorporated/74LVC1G17SE-7?qs=FRHfhEBFk1dzIcstjqNcyA%3D%3D"/>
<attribute name="MPN" value="74LVC1G17SE-7"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="MPN" value="GRM155R71H104KE14D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D8" library="CPDQT5V0HE-HF" package="CPDQT5V0HEHF" value="CPDQT5V0HE-HF">
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes DIODE ESD 5VWM 65W 0402/SOD-923F"/>
<attribute name="HEIGHT" value="0.42mm"/>
<attribute name="MANUFACTURER_NAME" value="Comchip Technology"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="CPDQT5V0HE-HF"/>
<attribute name="MOUSER_PART_NUMBER" value=""/>
<attribute name="MOUSER_PRICE-STOCK" value=""/>
<attribute name="MPN" value="CPDQT5V0HE-HF"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D9" library="CPDQT5V0HE-HF" package="CPDQT5V0HEHF" value="CPDQT5V0HE-HF">
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes DIODE ESD 5VWM 65W 0402/SOD-923F"/>
<attribute name="HEIGHT" value="0.42mm"/>
<attribute name="MANUFACTURER_NAME" value="Comchip Technology"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="CPDQT5V0HE-HF"/>
<attribute name="MOUSER_PART_NUMBER" value=""/>
<attribute name="MOUSER_PRICE-STOCK" value=""/>
<attribute name="MPN" value="CPDQT5V0HE-HF"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="rcl" package="R0603" value="470">
<attribute name="MPN" value="CR0603-FX-4700ELF"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="77"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="AP64060WU-7" package="SOT95P280X100-6N" value="AP64060WU-7">
<attribute name="DESCRIPTION" value="Switching Voltage Regulators DCDC Conv HV Buck TSOT26(STD) T&amp;R 3K"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="MANUFACTURER_NAME" value="Diodes Inc."/>
<attribute name="MANUFACTURER_PART_NUMBER" value="AP64060WU-7"/>
<attribute name="MOUSER_PART_NUMBER" value="621-AP64060WU-7"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Diodes-Incorporated/AP64060WU-7?qs=Li%252BoUPsLEntiZYjFw%252BCbiQ%3D%3D"/>
<attribute name="MPN" value="AP64060WU-7"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="sfe" package="0402-RES" value="22.1K">
<attribute name="MPN" value="CR0402-FX-2212GLF"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="sfe" package="0402-RES" value="133K">
<attribute name="MPN" value="RC0402FR-07133KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="NRS4018T100MDGJ" package="NRS4018T100MDGJ" value="NRS4018T100MDGJ">
<attribute name="DESCRIPTION" value="Fixed Inductors 4018 10uH 180mOhms +/-20%Tol 1200mA"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="MANUFACTURER_NAME" value="TAIYO YUDEN"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="NRS4018T100MDGJ"/>
<attribute name="MOUSER_PART_NUMBER" value="963-NRS4018T100MDGJ"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/TAIYO-YUDEN/NRS4018T100MDGJ?qs=PzICbMaShUeiyHfvjt6KEw%3D%3D"/>
<attribute name="MPN" value="NRS4018T100MDGJ"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="rcl" package="C0805" value="10uF">
<attribute name="MPN" value="GRM21BR61H106KE43K"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="88"/>
<attribute name="SPICEPREFIX" value="C"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0805" value="22uF">
<attribute name="MPN" value="CL21A226MQQNNNE"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08402"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="MPN" value="GRM155R71H104KE14D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="sfe" package="0402-CAP" value="100pF">
<attribute name="MPN" value="CC0402JRNPO9BN101"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="FM240A" package="DIOM5025X231N" value="FM240A">
<attribute name="DESCRIPTION" value="Diodes - General Purpose, Power, Switching GP Si Rectifier SMB,2A,40V"/>
<attribute name="HEIGHT" value="2.31mm"/>
<attribute name="MANUFACTURER_NAME" value="Rectron"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="FM240A"/>
<attribute name="MOUSER_PART_NUMBER" value="583-FM240A"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Rectron/FM240A?qs=7pEAo90IqNG7sknZwmLYhQ%3D%3D"/>
<attribute name="MPN" value="FM240A"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="FM240A" package="DIOM5025X231N" value="FM240A">
<attribute name="DESCRIPTION" value="Diodes - General Purpose, Power, Switching GP Si Rectifier SMB,2A,40V"/>
<attribute name="HEIGHT" value="2.31mm"/>
<attribute name="MANUFACTURER_NAME" value="Rectron"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="FM240A"/>
<attribute name="MOUSER_PART_NUMBER" value="583-FM240A"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Rectron/FM240A?qs=7pEAo90IqNG7sknZwmLYhQ%3D%3D"/>
<attribute name="MPN" value="FM240A"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="SMAJ40CAe3_TR13" package="SMAJ40CAE3TR13" value="SMAJ40CAE3_TR13">
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes TVS"/>
<attribute name="HEIGHT" value="3.05mm"/>
<attribute name="MANUFACTURER_NAME" value="Microchip"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="SMAJ40CAe3/TR13"/>
<attribute name="MOUSER_PART_NUMBER" value="494-SMAJ40CAE3/TR13"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Microchip-Technology/SMAJ40CAe3-TR13?qs=pU29NIZ4ZwCw3PnlxOleOw%3D%3D"/>
<attribute name="MPN" value="SMAJ40CAe3/TR13"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="SSM3J356R_LF" package="SOTFL95P240X88-3N" value="SSM3J356R,LF">
<attribute name="DESCRIPTION" value="MOSFET Small-signal MOSFET ID: -2A, VDSS: -60V"/>
<attribute name="HEIGHT" value="0.88mm"/>
<attribute name="MANUFACTURER_NAME" value="Toshiba"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="SSM3J356R,LF"/>
<attribute name="MOUSER_PART_NUMBER" value="757-SSM3J356RLF"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Toshiba/SSM3J356RLF?qs=lhkzy8lC%252BSsL%2F1yLGjMnQA%3D%3D"/>
<attribute name="MPN" value="SSM3J356R,LF"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Z1" library="MMSZ5231B-7-F" package="SOD3716X145N" value="MMSZ5231B-7-F">
<attribute name="DESCRIPTION" value="Zener Diode 5.1V 5% 500mW SOD123 Diodes Inc MMSZ5231B-7-F Zener Diode, 5.1V 5% 0.5 W SMT 2-Pin SOD-123"/>
<attribute name="HEIGHT" value="1.45mm"/>
<attribute name="MANUFACTURER_NAME" value="Diodes Inc."/>
<attribute name="MANUFACTURER_PART_NUMBER" value="MMSZ5231B-7-F"/>
<attribute name="MOUSER_PART_NUMBER" value="621-MMSZ5231B-F"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Diodes-Incorporated/MMSZ5231B-7-F?qs=2ygBApjwyeMh7Sf0YL1qSw%3D%3D"/>
<attribute name="MPN" value="MMSZ5231B-7-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="SparkFun-Capacitors" package="0805" value="22uF">
<attribute name="MPN" value="CL21A226MQQNNNE"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08402"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="SparkFun-Capacitors" package="0805" value="22uF">
<attribute name="MPN" value="CL21A226MQQNNNE"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08402"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="sfe" package="0402-RES" value="100K">
<attribute name="MPN" value="AC0402FR-07100KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="sfe" package="0402-RES" value="100K">
<attribute name="MPN" value="AC0402FR-07100KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D7" library="CPDQT5V0HE-HF" package="CPDQT5V0HEHF" value="CPDQT5V0HE-HF">
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes DIODE ESD 5VWM 65W 0402/SOD-923F"/>
<attribute name="HEIGHT" value="0.42mm"/>
<attribute name="MANUFACTURER_NAME" value="Comchip Technology"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="CPDQT5V0HE-HF"/>
<attribute name="MOUSER_PART_NUMBER" value=""/>
<attribute name="MOUSER_PRICE-STOCK" value=""/>
<attribute name="MPN" value="CPDQT5V0HE-HF"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="MPN" value="GRM155R71H104KE14D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Z3" library="MMSZ5231B-7-F" package="SOD3716X145N" value="MMSZ5231B-7-F">
<attribute name="DESCRIPTION" value="Zener Diode 5.1V 5% 500mW SOD123 Diodes Inc MMSZ5231B-7-F Zener Diode, 5.1V 5% 0.5 W SMT 2-Pin SOD-123"/>
<attribute name="HEIGHT" value="1.45mm"/>
<attribute name="MANUFACTURER_NAME" value="Diodes Inc."/>
<attribute name="MANUFACTURER_PART_NUMBER" value="MMSZ5231B-7-F"/>
<attribute name="MOUSER_PART_NUMBER" value="621-MMSZ5231B-F"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Diodes-Incorporated/MMSZ5231B-7-F?qs=2ygBApjwyeMh7Sf0YL1qSw%3D%3D"/>
<attribute name="MPN" value="MMSZ5231B-7-F"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP7" library="SparkFun-Jumpers" package="SMT-JUMPER_2_NC_PASTE_SILK" value="JUMPER-SMT_2_NC_PASTE_SILK">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC4" library="74LVC1G07GW_125" package="SOT65P212X110-5N" value="74LVC1G07GW,125">
<attribute name="DESCRIPTION" value="74LVC1G07 - Buffer with open-drain output@en-us"/>
<attribute name="HEIGHT" value="1.1mm"/>
<attribute name="MANUFACTURER_NAME" value="Nexperia"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="74LVC1G07GW,125"/>
<attribute name="MOUSER_PART_NUMBER" value="771-74LVC1G07GW-G"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Nexperia/74LVC1G07GW125?qs=me8TqzrmIYW763Mg%2FG86Uw%3D%3D"/>
<attribute name="MPN" value="74LVC1G07GW,125"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC6" library="MCP2542FD-E_SN" package="SOIC127P600X175-8N" value="MCP2542FD-E_SN">
<attribute name="DESCRIPTION" value="Microchip MCP2542FD-E/SN, CAN Transceiver 8Mbit/s 1-Channel CAN, ISO 11898-2, ISO 11898-5, ISO/DIS11898-2, 8-Pin SOIC"/>
<attribute name="HEIGHT" value="1.75mm"/>
<attribute name="MANUFACTURER_NAME" value="Microchip"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="MCP2542FD-E/SN"/>
<attribute name="MOUSER_PART_NUMBER" value="579-MCP2542FD-E/SN"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Microchip-Technology-Atmel/MCP2542FD-E-SN?qs=qdgZG5p0FZ5pNizBl1u80Q%3D%3D"/>
<attribute name="MPN" value="MCP2542FD-E/SN"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="MPN" value="GRM155R71H104KE14D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D12" library="SparkFun-DiscreteSemi" package="SOT23-3" value="PESD1CAN">
<attribute name="MPN" value="VCAN36A2-03S-E3-08"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-12501"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="rcl" package="R1206" value="60">
<attribute name="MPN" value="RC1206FR-0760R4L"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="19"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="sfe" package="0402-CAP" value="100pF">
<attribute name="MPN" value="CC0402JRNPO9BN101"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="sfe" package="0402-CAP" value="100pF">
<attribute name="MPN" value="CC0402JRNPO9BN101"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="rcl" package="R1206" value="60">
<attribute name="MPN" value="RC1206FR-0760R4L"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="19"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="D10" library="CPDQT5V0HE-HF" package="CPDQT5V0HEHF" value="CPDQT5V0HE-HF">
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes DIODE ESD 5VWM 65W 0402/SOD-923F"/>
<attribute name="HEIGHT" value="0.42mm"/>
<attribute name="MANUFACTURER_NAME" value="Comchip Technology"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="CPDQT5V0HE-HF"/>
<attribute name="MOUSER_PART_NUMBER" value=""/>
<attribute name="MOUSER_PRICE-STOCK" value=""/>
<attribute name="MPN" value="CPDQT5V0HE-HF"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D11" library="CPDQT5V0HE-HF" package="CPDQT5V0HEHF" value="CPDQT5V0HE-HF">
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes DIODE ESD 5VWM 65W 0402/SOD-923F"/>
<attribute name="HEIGHT" value="0.42mm"/>
<attribute name="MANUFACTURER_NAME" value="Comchip Technology"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="CPDQT5V0HE-HF"/>
<attribute name="MOUSER_PART_NUMBER" value=""/>
<attribute name="MOUSER_PRICE-STOCK" value=""/>
<attribute name="MPN" value="CPDQT5V0HE-HF"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="sfe" package="0402-RES" value="10K">
<attribute name="MPN" value="AC0402FR-1310KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="sfe" package="0402-RES" value="10K">
<attribute name="MPN" value="AC0402FR-1310KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L4" library="SRF4532-110Y" package="SRF4532101Y" value="SRF4532-110Y">
<attribute name="DESCRIPTION" value="Bourns Type 4532 Wire-wound SMD Inductor with a Ferrite Core, 11 uH -30  +50% Wire-Wound 300mA Idc"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="MANUFACTURER_NAME" value="Bourns"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="SRF4532-110Y"/>
<attribute name="MOUSER_PART_NUMBER" value="652-SRF4532-110Y"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Bourns/SRF4532-110Y?qs=u649AIwumF8o5t6hcAfmlw%3D%3D"/>
<attribute name="MPN" value="SRF4532-110Y"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="MPN" value="GRM155R71H104KE14D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="sfe" package="0402-CAP" value="4.7nF">
<attribute name="MPN" value="GRM155R71H472JA01D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC5" library="SN65C3221EPWR" package="SOP65P640X120-16N" value="SN65C3221EPWR">
<attribute name="DESCRIPTION" value="3-V To 5.5-V Single Channel RS-232 1 Mbit/s Line Driver/Receiver"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="MANUFACTURER_NAME" value="Texas Instruments"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="SN65C3221EPWR"/>
<attribute name="MOUSER_PART_NUMBER" value="595-SN65C3221EPWR"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Texas-Instruments/SN65C3221EPWR?qs=6siQ5y5nVCwNDulozFTH8A%3D%3D"/>
<attribute name="MPN" value="SN65C3221EPWR"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="sfe" package="0402-RES" value="10K">
<attribute name="MPN" value="AC0402FR-1310KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="sfe" package="0402-RES" value="10K">
<attribute name="MPN" value="AC0402FR-1310KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D13" library="CPDQT5V0HE-HF" package="CPDQT5V0HEHF" value="CPDQT5V0HE-HF">
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes DIODE ESD 5VWM 65W 0402/SOD-923F"/>
<attribute name="HEIGHT" value="0.42mm"/>
<attribute name="MANUFACTURER_NAME" value="Comchip Technology"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="CPDQT5V0HE-HF"/>
<attribute name="MOUSER_PART_NUMBER" value=""/>
<attribute name="MOUSER_PRICE-STOCK" value=""/>
<attribute name="MPN" value="CPDQT5V0HE-HF"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D14" library="CPDQT5V0HE-HF" package="CPDQT5V0HEHF" value="CPDQT5V0HE-HF">
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes DIODE ESD 5VWM 65W 0402/SOD-923F"/>
<attribute name="HEIGHT" value="0.42mm"/>
<attribute name="MANUFACTURER_NAME" value="Comchip Technology"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="CPDQT5V0HE-HF"/>
<attribute name="MOUSER_PART_NUMBER" value=""/>
<attribute name="MOUSER_PRICE-STOCK" value=""/>
<attribute name="MPN" value="CPDQT5V0HE-HF"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="MPN" value="GRM155R71H104KE14D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="MPN" value="GRM155R71H104KE14D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="MPN" value="GRM155R71H104KE14D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="MPN" value="GRM155R71H104KE14D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="MPN" value="GRM155R71H104KE14D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="sfe" package="0402-CAP" value="100pF">
<attribute name="MPN" value="CC0402JRNPO9BN101"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D15" library="SparkFun-DiscreteSemi" package="SOT23-3" value="PESD1CAN">
<attribute name="MPN" value="VCAN36A2-03S-E3-08"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-12501"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="sfe" package="0402-CAP" value="100pF">
<attribute name="MPN" value="CC0402JRNPO9BN101"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L5" library="sfe" package="C0402" value="100">
<attribute name="MPN" value="MFBM1V1005-101-R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L3" library="sfe" package="C0402" value="100">
<attribute name="MPN" value="MFBM1V1005-101-R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="SparkFun-Jumpers" package="SMT-JUMPER_2_NC_PASTE_SILK" value="JUMPER-SMT_2_NC_PASTE_SILK">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP5" library="SparkFun-Jumpers" package="SMT-JUMPER_2_NC_PASTE_SILK" value="JUMPER-SMT_2_NC_PASTE_SILK">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Jumpers" package="SMT-JUMPER_2_NC_PASTE_SILK" value="JUMPER-SMT_2_NC_PASTE_SILK">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun-Jumpers" package="SMT-JUMPER_2_NC_PASTE_SILK" value="JUMPER-SMT_2_NC_PASTE_SILK">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP9" library="SparkFun-Jumpers" package="SMT-JUMPER_3_1-NC_PASTE_SILK" value="JUMPER-SMT_3_1-NC_PASTE_SILK">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP10" library="SparkFun-Jumpers" package="SMT-JUMPER_2_NC_PASTE_SILK" value="JUMPER-SMT_2_NC_PASTE_SILK">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP11" library="SparkFun-Jumpers" package="SMT-JUMPER_2_NC_PASTE_SILK" value="JUMPER-SMT_2_NC_PASTE_SILK">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Jumpers" package="SMT-JUMPER_2_NO_SILK" value="JUMPER-SMT_2_NO_SILK">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP6" library="SparkFun-Jumpers" package="SMT-JUMPER_2_NC_PASTE_SILK" value="JUMPER-SMT_2_NC_PASTE_SILK">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="sfe" package="0402-RES" value="100K">
<attribute name="MPN" value="AC0402FR-07100KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="sfe" package="0402-RES" value="51K">
<attribute name="MPN" value="RC0402JR-0751KL"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="CPDQT5V0HE-HF" package="CPDQT5V0HEHF" value="CPDQT5V0HE-HF">
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes DIODE ESD 5VWM 65W 0402/SOD-923F"/>
<attribute name="HEIGHT" value="0.42mm"/>
<attribute name="MANUFACTURER_NAME" value="Comchip Technology"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="CPDQT5V0HE-HF"/>
<attribute name="MOUSER_PART_NUMBER" value=""/>
<attribute name="MOUSER_PRICE-STOCK" value=""/>
<attribute name="MPN" value="CPDQT5V0HE-HF"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC3" library="LM321LVIDCKR" package="SOT65P210X110-5N" value="LM321LVIDCKR">
<attribute name="DESCRIPTION" value="1-Channel industry standard low voltage operational amplifier"/>
<attribute name="HEIGHT" value="1.1mm"/>
<attribute name="MANUFACTURER_NAME" value="Texas Instruments"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="LM321LVIDCKR"/>
<attribute name="MOUSER_PART_NUMBER" value="595-LM321LVIDCKR"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Texas-Instruments/LM321LVIDCKR?qs=qSfuJ%252Bfl%2Fd6RcyTOjkRx5Q%3D%3D"/>
<attribute name="MPN" value="LM321LVIDCKR"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP8" library="SparkFun-Jumpers" package="SMT-JUMPER_2_NO_SILK" value="JUMPER-SMT_2_NO_SILK">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="sfe" package="0402-CAP" value="0.1uF">
<attribute name="MPN" value="GRM155R71H104KE14D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D6" library="CPDQT5V0HE-HF" package="CPDQT5V0HEHF" value="CPDQT5V0HE-HF">
<attribute name="DESCRIPTION" value="ESD Suppressors / TVS Diodes DIODE ESD 5VWM 65W 0402/SOD-923F"/>
<attribute name="HEIGHT" value="0.42mm"/>
<attribute name="MANUFACTURER_NAME" value="Comchip Technology"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="CPDQT5V0HE-HF"/>
<attribute name="MOUSER_PART_NUMBER" value=""/>
<attribute name="MOUSER_PRICE-STOCK" value=""/>
<attribute name="MPN" value="CPDQT5V0HE-HF"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="rcl" package="R0603" value="470">
<attribute name="MPN" value="CR0603-FX-4700ELF"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="77"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
<element name="Z2" library="MM3Z3V6T1G" package="SOD2512X110N" value="DNP">
<attribute name="DESCRIPTION" value="ON Semiconductor MM3Z3V6T1G Zener Diode, 3.6V 5% 200 mW SMT 2-Pin SOD-323"/>
<attribute name="HEIGHT" value="1.1mm"/>
<attribute name="MANUFACTURER_NAME" value="onsemi"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="MM3Z3V6T1G"/>
<attribute name="MOUSER_PART_NUMBER" value="863-MM3Z3V6T1G"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/onsemi/MM3Z3V6T1G?qs=HVbQlW5zcXWbZo78nv8gqg%3D%3D"/>
<attribute name="MPN" value="MM3Z3V6T1G"/>
<attribute name="NAME"/>
<attribute name="POPULATE" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="rcl" package="R0603" value="240">
<attribute name="MPN" value="RK73B1JTTD241J"/>
<attribute name="NAME"/>
<attribute name="POPULARITY" value="77"/>
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="J1" pad="24"/>
<contactref element="J1" pad="9"/>
<contactref element="D2" pad="2"/>
<contactref element="IC1" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="D8" pad="2"/>
<contactref element="U1" pad="3"/>
<contactref element="C11" pad="1"/>
<contactref element="D9" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="IC2" pad="2"/>
<contactref element="D3" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="C6" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="D4" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="D7" pad="2"/>
<contactref element="C10" pad="1"/>
<contactref element="Z3" pad="2"/>
<contactref element="IC4" pad="3"/>
<contactref element="D11" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="D10" pad="2"/>
<contactref element="IC6" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="IC6" pad="8"/>
<contactref element="C23" pad="2"/>
<contactref element="C12" pad="1"/>
<contactref element="D12" pad="3"/>
<contactref element="C15" pad="2"/>
<contactref element="IC5" pad="1"/>
<contactref element="C22" pad="2"/>
<contactref element="C21" pad="2"/>
<contactref element="IC5" pad="14"/>
<contactref element="C20" pad="2"/>
<contactref element="D14" pad="2"/>
<contactref element="D13" pad="2"/>
<contactref element="C19" pad="2"/>
<contactref element="C13" pad="1"/>
<contactref element="D15" pad="3"/>
<contactref element="J2" pad="2"/>
<contactref element="D5" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="IC3" pad="2"/>
<contactref element="C9" pad="1"/>
<contactref element="D6" pad="2"/>
<contactref element="Z2" pad="2"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="N$69">
</signal>
<signal name="N$17">
</signal>
<signal name="N$18">
</signal>
<signal name="N$1">
</signal>
<signal name="N$2">
</signal>
<signal name="N$3">
</signal>
<signal name="N$4">
</signal>
<signal name="N$6">
</signal>
<signal name="N$7">
</signal>
<signal name="N$8">
</signal>
<signal name="N$9">
</signal>
<signal name="N$10">
</signal>
<signal name="N$12">
</signal>
<signal name="N$20">
</signal>
<signal name="N$21">
</signal>
<signal name="VCC">
<contactref element="J1" pad="8"/>
<contactref element="D2" pad="1"/>
<contactref element="L2" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="C10" pad="2"/>
<contactref element="IC4" pad="5"/>
<contactref element="R12" pad="1"/>
<contactref element="R13" pad="1"/>
<contactref element="C18" pad="1"/>
<contactref element="IC6" pad="5"/>
<contactref element="R14" pad="1"/>
<contactref element="R15" pad="1"/>
<contactref element="IC5" pad="15"/>
<contactref element="C20" pad="1"/>
<contactref element="IC5" pad="16"/>
<contactref element="IC5" pad="12"/>
</signal>
<signal name="VIN">
<contactref element="J1" pad="10"/>
<contactref element="D1" pad="1"/>
</signal>
<signal name="SW">
<contactref element="L2" pad="2"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="V_BATT">
<contactref element="IC1" pad="4"/>
<contactref element="C4" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="U1" pad="5"/>
<contactref element="R6" pad="1"/>
<contactref element="IC6" pad="3"/>
<contactref element="C17" pad="1"/>
<contactref element="IC3" pad="5"/>
<contactref element="C9" pad="2"/>
</signal>
<signal name="SYNC_IN_INT">
<contactref element="R10" pad="1"/>
<contactref element="D7" pad="1"/>
<contactref element="Z3" pad="1"/>
<contactref element="IC4" pad="2"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="P10_FSYNC">
<contactref element="D8" pad="1"/>
<contactref element="U1" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="JP7" pad="2"/>
<contactref element="IC4" pad="4"/>
</signal>
<signal name="SYNC_IN">
<contactref element="R10" pad="2"/>
<contactref element="JP9" pad="3"/>
</signal>
<signal name="SYNC_OUT_INT">
<contactref element="U1" pad="4"/>
<contactref element="D9" pad="1"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="SYNC_OUT">
<contactref element="R9" pad="2"/>
<contactref element="JP9" pad="1"/>
</signal>
<signal name="EXT_VIN_G">
<contactref element="Q1" pad="1"/>
<contactref element="Z1" pad="2"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="EXT_VIN_INT">
<contactref element="Z1" pad="1"/>
<contactref element="Q1" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="IC2" pad="5"/>
<contactref element="IC2" pad="4"/>
</signal>
<signal name="EXT_VIN">
<contactref element="Q1" pad="3"/>
<contactref element="D4" pad="2"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="EXT_VIN_BST">
<contactref element="IC2" pad="1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="EXT_VIN_SW">
<contactref element="IC2" pad="6"/>
<contactref element="L1" pad="1"/>
<contactref element="D3" pad="1"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="EXT_VIN_OUT">
<contactref element="L1" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="D1" pad="2"/>
</signal>
<signal name="EXT_VIN_FB">
<contactref element="IC2" pad="3"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="P10_FSYNC_INT">
<contactref element="J1" pad="14"/>
<contactref element="JP7" pad="1"/>
</signal>
<signal name="CAN_TX">
<contactref element="IC6" pad="1"/>
<contactref element="R12" pad="2"/>
<contactref element="D10" pad="1"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="CAN_RX">
<contactref element="D11" pad="1"/>
<contactref element="IC6" pad="4"/>
<contactref element="R13" pad="2"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="CANL">
<contactref element="C23" pad="1"/>
<contactref element="D12" pad="2"/>
<contactref element="L4" pad="3"/>
<contactref element="J2" pad="4"/>
<contactref element="JP11" pad="1"/>
</signal>
<signal name="CANH">
<contactref element="C12" pad="2"/>
<contactref element="D12" pad="1"/>
<contactref element="L4" pad="2"/>
<contactref element="J2" pad="3"/>
<contactref element="JP10" pad="2"/>
</signal>
<signal name="CAN_S">
<contactref element="R17" pad="2"/>
<contactref element="R16" pad="1"/>
<contactref element="C15" pad="1"/>
</signal>
<signal name="C1+">
<contactref element="IC5" pad="2"/>
<contactref element="C14" pad="1"/>
</signal>
<signal name="C1-">
<contactref element="C14" pad="2"/>
<contactref element="IC5" pad="4"/>
</signal>
<signal name="C2-">
<contactref element="IC5" pad="6"/>
<contactref element="C16" pad="1"/>
</signal>
<signal name="C2+">
<contactref element="IC5" pad="5"/>
<contactref element="C16" pad="2"/>
</signal>
<signal name="V-">
<contactref element="IC5" pad="7"/>
<contactref element="C21" pad="1"/>
</signal>
<signal name="V+">
<contactref element="C22" pad="1"/>
<contactref element="IC5" pad="3"/>
</signal>
<signal name="RXI">
<contactref element="IC5" pad="8"/>
<contactref element="L5" pad="1"/>
</signal>
<signal name="RS232_RXI">
<contactref element="D14" pad="1"/>
<contactref element="IC5" pad="9"/>
<contactref element="R15" pad="2"/>
<contactref element="JP5" pad="2"/>
</signal>
<signal name="RS232_TXO">
<contactref element="D13" pad="1"/>
<contactref element="IC5" pad="11"/>
<contactref element="R14" pad="2"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="TXO">
<contactref element="IC5" pad="13"/>
<contactref element="L3" pad="1"/>
</signal>
<signal name="EXT_RXI">
<contactref element="L5" pad="2"/>
<contactref element="C19" pad="1"/>
<contactref element="D15" pad="2"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="EXT_TXO">
<contactref element="L3" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="D15" pad="1"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="RS232_RXI_INT">
<contactref element="JP5" pad="1"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="RS232_TXO_INT">
<contactref element="J1" pad="5"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="CAN_RX_INT">
<contactref element="J1" pad="4"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="CAN_TX_INT">
<contactref element="J1" pad="2"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="SYNC">
<contactref element="JP9" pad="2"/>
<contactref element="J2" pad="8"/>
</signal>
<signal name="CANH_INT">
<contactref element="IC6" pad="7"/>
<contactref element="L4" pad="1"/>
</signal>
<signal name="CANL_INT">
<contactref element="L4" pad="4"/>
<contactref element="IC6" pad="6"/>
</signal>
<signal name="CANH_J">
<contactref element="JP10" pad="1"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="CANL_J">
<contactref element="JP11" pad="2"/>
<contactref element="R17" pad="1"/>
</signal>
<signal name="CAN_TX_INT_2">
<contactref element="JP2" pad="1"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="P6_ADC_INT">
<contactref element="J1" pad="7"/>
<contactref element="JP6" pad="1"/>
</signal>
<signal name="P6_ADC">
<contactref element="JP6" pad="2"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="AIN">
<contactref element="J2" pad="7"/>
<contactref element="R4" pad="2"/>
<contactref element="JP8" pad="2"/>
</signal>
<signal name="AIN_INT">
<contactref element="R4" pad="1"/>
<contactref element="D5" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="IC3" pad="1"/>
<contactref element="Z2" pad="1"/>
</signal>
<signal name="AIN_S">
<contactref element="JP8" pad="1"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="AIN_OUT">
<contactref element="IC3" pad="3"/>
<contactref element="IC3" pad="4"/>
<contactref element="D6" pad="1"/>
<contactref element="R5" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
